# 2nd Division

If loss of normal communications, AC, DL and CMs turn on radio and monitor. The first Net will be the AC to DL Net. Then the DL to BC Net. Lastly the BC to CM Net.

AC – Default – The ACs always monitors CCAREA 025

GM-15 PRO

D. Wait **Off** [Menu, 06, Menu, up arrow, Menu, exit]

 CCAREA 025

DL- Default - Waiting for AC Net

GM-15 PRO

D. Wait **Off** [Menu, 06, Menu, up arrow, Menu, exit]

CCAREA 025

 BC 085

DL SWITCH to BC and enable D.Wait and run the BC Net

DL GM-15 PRO

D.Wait **On** [Menu, 06, Menu, up arrow, Menu, exit]

DL 015 (CCAREA 025 to DL 015)

 BC 061

BC – Default – Waiting for DL Net

BC MU-5

D. Wait **On** [Menu, 06, Menu, up arrow, Menu, exit]

 BC 007

 DL 040

BC SWITCH to CM set D.Wait **On** and run the CM Net

BC MU-5

D. Wait **On** [Menu, 06, Menu, up arrow, Menu, exit]

DL 040

 CM 010 (BC 007 to CM 010)

The community radio settings do not change. And they are locked by default. By default, the community radio can receive CCAREA traffic, and both transmit and receive BC and nearby community members traffic.

CM MU-5 – Waiting for BC Net

CM 010

CCAREA 021